1. Shutdown Robot.
2. Remote Desktop to 192.168.10.100/159/179/126/151/175/150/200
3. Close the executed applocations, shutdown each remote.
4. Shutdown robots physically.
5. Log off picking station and shutdown it.
6. Click ‘Offline’ to log off picking station.
7. Swipe left on the screen, click the windowns icon. Then swipe up on the screen, click the ‘command prompt’（command windown）, then close it.
8. Then power off the PC.
9. Shutdown RCS server.
10. When login server, choose Not listed.
11. Input username ‘root’, password ‘111111’ (If the terminal was opened before, just go to step 7)
12. Click ‘Applications’ on the left corner, select ‘Terminal’ to open a command window.
13. Input ‘cd /opt’, press enter
14. Input ‘cd walle’, press enter
15. Input ‘cd deploy’, press enter
16. Input ‘sh stopall.sh’, press enter to stop RCS program.
17. Close the terminal window.
18. Click ‘root’ on the right corner, click ‘Power Off’ to shutdown server.
19. Shutdown Dispatcher server (Suggest don’t showdown the server unless have to do it)
20. Go to the opened eclipse, click the red block to stop the interface program.
21. Close eclipse.
22. Click root button on the right corner,click ‘Quit…’ to shutdown server.